Software
1. Copy the software file into USB root directory, Reminder: do not change file name£¨v100.bin)
2. Insert U disk into New SH-1000HD USB interface
3. Move cursor to "Software"
4. Press and hold the right button for 2 seconds
5. Release right button 
6. Waiting the finder auto restart

TP List
1. Copy the defaultdb file into USB root directory, Reminder: do not change file name£¨defaultdb)
2. Insert U disk into New SH-1000HD USB interface
3. Move cursor to "DATA"
4. Press and hold the right button for 2 seconds
5. Release right button 
6. Waiting the finder auto restart
